Michael Gontarek

CS-350

Emerging Sys Arch & Tech

Southern New Hampshire University

Milestone Two Submission

• How does the macro UART\_DATA\_BINARY impact the UART?

* UART\_DATA\_BINARY prevents data processing during read/ write steps.

• How does the macro UART\_RETURN\_FULL impact the UART?

* Lets you know when buffer is full

• What driver call would you use to write 10 characters out of the UART?

* CONFIG\_TI\_DRIVERS\_UART\_COUNT

• What is the driver call to turn off LED 0?

* CONFIG\_GIPO\_LED\_0

• What is the UART baud rate?

* 115200